C42 REPAIRING / RENOVATING / CONSERVING CONCRETE

 To be read with Preliminaries / General conditions.

J40/310333333333

3100110101010293I8E4844444

310 REPAIR MORTAR

* Type : Copolymer cementitious mortar
* Manufacturer : RIW Limited, Arc House, Terrace Road South, Binfield, RG42 4PZ.

 Tel : 01344 397777 Fax : 01344 862010

 E-mail : technical@riw.co.uk Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Cementfill HB

* Application thickness : 5mm minimum, 80mm maximum per layer.
* Primer : Not required

*or : for highly porous substrates*

* Primer : RIW Cementseal Primer